# Model 647 Changelog

NOTE, when updating between versions where any digit but the last has changed:
- New settings have been added
- The update will set reset the unit to Factory Default settings, except for IP settings
- Previous settings will automatically be recalled after Factory Defaults are loaded
- This will take ~30 seconds after the unit has been updated, and it will reboot after
- Any new settings that didn't exist in the previous firmware will be at their respective defaults

How to update firmware:
- Access the Admin webpage
- Click "Select Firmware File..."
- Select the firmware (.bin file)
- Click "Update Firmware"
- Wait for update to complete

=== Rev 1.0.0.7 ===		
- Fix issue with a bug in the LCD Menu

=== Rev 1.0.0.6 ===
- Enable pullups for SD pins

=== Rev 1.0.0.5 ===
- Fix NRSC filter coefficients

=== Rev 1.0.0.4 ===
-  Fix HTTP Port not setting properly

=== Rev 1.0.0.3 ===
- Adjust header meter visibility

=== Rev 1.0.0.2 ===
- Fix Alarm Status for Station Rotation

=== Rev 1.0.0.1 ===
- Remove unnecessary items from MIB file

=== Rev 1.0.0.0 ===
- Official Firmware Release