# Model 704 Changelog

NOTE, when updating between versions where any digit but the last has changed:
- New settings have been added
- The update will set reset the unit to Factory Default settings, except for IP settings
- Previous settings will automatically be recalled after Factory Defaults are loaded
- This will take ~30 seconds after the unit has been updated, and it will reboot after
- Any new settings that didn't exist in the previous firmware will be at their respective defaults

How to update firmware:
- Access the Admin webpage
- Click "Select Firmware File..."
- Select the firmware (.bin file)
- Click "Update Firmware"
- Wait for update to complete

=== Rev 1.0.0.15 ===
- Fix issue with TCP sockets for reliable reconnection

=== Rev 1.0.0.14 ===
- Fixed issue with '&' in the PS or RT field not displaying properly

=== Rev 1.0.0.13 ===
- Fixed issue with RT+ tagging when using the RTP command
- Improved RT+ group timing so radios will more likely show RT and RT+ change at the same time.
- Fixed RT+ tags not clearing when RT Default is loaded

=== Rev 1.0.0.12 ===
- Added RTP command for RadioText+

=== Rev 1.0.0.9 ===
- Fix issue with UDP connections

=== Rev 1.0.0.8 ===
- Fix issue with TCP connections

=== Rev 1.0.0.7 ===
- Fix PI remapping occurring when RDS mode is not RBDS

=== Rev 1.0.0.6 ===
- Fix issue with DPS not saving when using the DPSTEXT command via Telnet
- Fix issue when changing TCP ports and the unit not responding

=== Rev 1.0.0.5 ===
- Fix issue with webpage TCP led not staying active when connection is established

=== Rev 1.0.0.4 ===
- Fix phase slider

=== Rev 1.0.0.3 ===
- Fix pilot menu not properly reflecting pilot lock

=== Rev 1.0.0.2 ===
- Update pilot locking configuration

=== Rev 1.0.0.1 ===
- Update pilot locking configuration

=== Rev 1.0.0.0 ===
- Initial release
