*****************************
*                           *
* MODEL 637 FIRMWARE UPDATE *
*                           *
*****************************

--- BEFORE UPDATING FIRMWARE ---

Backup the hardware profile via the admin webpage before updating the firmware.
Then, run the Firmware Update executable and follow the on screen directions.
You can then upload your hardware profile to restore your settings.

--- AFTER UPDATING FIRMWARE ---

Run the Webpage Uploader executable to upload the webpage files to the newer version.


REV 1.0.0.2
- Fixed an issue with sending daily log.
- Fixed an issue with failed to sending alarm emails in some certain condition.

REV 1.0.0.3
- Fixed multiple issue with SNMP.

REV 1.0.0.4
- Added a lower streaming rate option.

REV 1.1.0.0
- Added TLS1.2 support to SMTP client.
- Expanded presets to 30, preset name length to 16

REV 1.1.0.1
- Hotfix for an issue introduced in 1.1.0.0. If the alarm log is large,
  loading the log on the webpage would cause the webpages to become
  unresponsive.

REV 1.1.0.2
- Fixed a bug with SMTP that could result in emails not sending for some SMTP servers
- Fixed a TLS issue with some SMTP servers (yahoo)

REV 1.1.0.4
- UI changes

REV 1.1.0.5
- Fixed a bug with the Security Enable checkbox not working correctly on the Admin webpage
- Fixed issue with RSSI level showing lower than it should if you select a preset while the front panel is on the tuner menu

REV 1.1.0.6
- Fixed not being able to set several settings via SNMP (frequency, deemphasis, bandwidth, source, gain)
- Changed time server poll interval to 1 hour for more accurate alarm log timestamping

REV 1.2.0.0
- Added time (12HR/24HR) and date (mm/dd/yy, dd/mm/yy) format settings

REV 1.2.0.1
- Improved web server resilience when connected to over a poor connection:
  Tested on a remote device with browser throttling ("Fast 3G" preset) and 10% each of: packet drop, duplication, out of order, tampering.